
Declaration of Conformity (DoC)

We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	[bookmark: _GoBack]Smart Phone 

	Trademark： 
	Blackview / OSCAL

	Model Number(s):
	BL7000, PILOT 3, BL7000 Pro




(Name of product, type or model, batch or serial number)

(Name of product, type or model, batch or serial number)

System components:
PIFA Antenna:BT/Wi-Fi2.4G:2.2dBi; WIFI5G:2.7dBi;
GSM900: -1.58dBi/DCS1800: 0.76dBi; WCDMABandⅠ: 1.12dBi,BandⅧ: -1.58dBi;
LTE: Band 1: 1.12dBi; Band 3: 0.76dBi; Band 7: 1.61dBi; Band 8: -1.58dBi; Band 20: -1.57dBi; 
Band 28: -1.93dBi; Band 40: 1.46dBi; Band 41: 1.54dBi 
NR: N1: 1.12dBi; N3: 0.76dBi; N8: -1.58dBi; N20: -1.57dBi; N28: -1.93dBi; 
N40: 1.46dBi; N41: 1.54dBi; N77: 2.21dBi;N78: 2.23dBi
Adapter :
Model: QZ-04501EC00
Input: 100-240V~50/60Hz 1.2A
Output: 5.0V 3.0A 15.0W or 9.0V 3.0A 27.0W
     or 12.0V 2.5A 30.0W or 15.0V 2.0A 30.0W
     or 20.0V 2.25A 45.0W Max
(PPS) 5.0V-11.0V 3.0A 33.0W Max
(PPS) 5.0V-20.0V 2.25A 45.0W Max
Manufacturer: Guangdong Quanzhi Technology Co., Ltd

RechargeableLi-ionBattery:
Model:Li386284HTT; Specification:DC 3.87V, 7500mAh,29.025Wh;
Manufacturer: Shenzhen Huatiantong Technology Co., Ltd

Hardware Version: F216_MAIN_PCB_V1.0
Software Version: BL7000_NEU_F216_V1.0/PILOT 3_NEU_F216_V1.0/
BL7000 Pro_NEU_F216_V1.0
[image: lQDPKGn_5qeCy_fNC9DND8CweI2_Mb1UH1AHvmZGdMr8AA_4032_3024]
The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

HEALTH & SAFETY (Art. 3(1)(a)):

EN 50360:2017+A1:2023
EN 50566:2017+A1:2023
EN 62209-1:2016
EN 62209-2:2010
EN 62479: 2010
EN IEC 62368-1:2020+A11:2020
EMC (Art. 3(1)(b)):

[bookmark: OLE_LINK187][bookmark: OLE_LINK188]ETSI EN 301 489-1 V2.2.3 (2019-11)
ETSI EN 301 489-3 V2.3.2 (2023-01)
ETSI EN 301 489-17 V3.3.1 (2024-09)
ETSI EN 301 489-19 V2.2.1 (2022-09)
ETSI EN 301 489-52 V1.2.1 (2021-11)
EN 55032:2015+A1:2020	
EN 55035:2017+A11:2020
EN IEC 61000-3-2:2019+A1:2021
EN 61000-3-3:2013+A2:2021

Radio Spectrum (Article 3.2):

ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 300 440 V2.2.1 (2018-07)
ETSI EN 301 511 V12.5.1 (2017-03)
ETSI EN 301 908-1 V15.2.1 (2023-01)
ETSI EN 301 908-2 V13.1.1 (2020-06)
ETSI EN 301 908-13 V13.2.1 (2022-02)
ETSI EN 301 908-25 V15.1.1 (2024-10)
ETSI EN 303 413 V1.2.1 (2021-04)
ETSI EN 303 345-1 V1.1.1 (2019-06)
ETSI EN 303 345-3 V1.1.1 (2021-06)
ETSI EN 300 330 V2.1.1 (2017-02)


The submitted samples of the above equipment has been tested and found to comply with the following European 
Directives: RoHS Directive 2011/65/EU & (EU) 2015/863






NOTIFIEDBODY:
[bookmark: Name:DERYCOM_CERTIFICATION_SERVICES,_INC]Name: LGAl Technological Center S.A. (APPLUS)

Address: Campus UAB. Ronda de la Font del Carme s/n08193 Bellaterra, Barcelona (Spain)

IdentificationNumber: 0370

EU-type examination certificate number: No. 0370-RED-11551



RF Specification:

	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	0.6dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	8.26dBm

	WIFI 802.11b/g/
n(HT20/40)
	802.11b/g/n(20MHz): 2412~2472MHz;
802.11n(40MHz):2422~2462MHz
	16.22dBm

	Wi-Fi
5.2G(802.11a/n20/n40/ac20/ac40/ac80)
	802.11a/ n20/ac20:5180MHz~5240MHz
802.11 n40/ac40:5190MHz~5230MHz
802.11 ac80:5210MHz
	11.7dBm

	Wi-Fi
5.8G(802.11a/n20/n40/ac20/ac40/ac80)
	802.11a/ n20/ac20:5745MHz~5825MHz
802.11 n40/ac40:5755MHz~5795MHz
802.11ac80:5775MHz
	12.17dBm

	GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;
RX(Downlink):925M‐960MHZ
	33.21 dBm

	GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;
RX(Downlink):1805M‐1880MHZ
	30.41 dBm 

	WCDMA B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	23.25 dBm 

	WCDMA B8
	TX(Uplink): 880-915MHz;
RX(Downlink):925-960MHz
	22.71 dBm 

	LTE FDD B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	24.06dBm 

	LTE FDD B3
	TX(Uplink) :1710-1785MHz;
RX(Downlink):1805-1880MHz
	24.33 dBm 

	LTE FDD B7
	TX(Uplink) :2500-2570MHz;
RX(Downlink):2620-2690MHz
	24.29dBm 

	LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz
RX(Downlink): 925 MHz to 960 MHz
	24.24dBm 

	LTE FDD B20
	TX(Uplink): 832MHz~862MHz;
RX(Downlink):791MHz~821MHz
	24.28 dBm

	LTE FDD B28
	TX(Uplink):  703 MHz to 748MHz
RX(Downlink): 758 MHz to 803 MHz
	24.41 dBm

	LTE TDD B40
	Uplink & Downlink: 2300 MHz to 2400 MHz
	22.79 dBm

	LTE TDD B41
	Uplink & Downlink: 2496 MHz to 2690 MHz
	26.54 dBm

	NR FDD n1:
	Uplink: 1920 MHz to 1980MHz
Downlink: 2110 MHz to 2170 MHz
	24.28 dBm

	NR FDD n3:
	Uplink: 1710 MHz to 1785 MHz
Downlink: 1805 MHz to 1880 MHz
	24.1dBm

	NR FDD n8: 
	Uplink: 880 MHz to 915 MHz
Downlink: 925 MHz to 960 MHz
	23.92 dBm

	NR FDD n20: 
	Uplink: 832 MHz to 862 MHz
Downlink: 791 MHz to 821 MHz
	23.97 dBm

	NR FDD n28: 
	Uplink: 703 MHz to 748 MHz
Downlink: 758 MHz to 803 MHz
	23.29 dBm

	NR TDD n40:
	Uplink & Downlink: 2300 MHz to 2400 MHz
	24.37 dBm

	NR TDD n41:
	Uplink & Downlink: 2496 MHz to 2690 MHz
	27.95 dBm

	NR TDD n77: 
	Uplink & Downlink: 3300 MHz to 4200 MHz
	27.59 dBm

	NR TDD n78
	Uplink & Downlink: 3300 MHz to 3800 MHz
	27.5 dBm

	NFC
	13.56MHz
	11.16 dBuA/m@10m 

	FM
	Rx(Downlink): 87.5MHz~108MHz
	--

	GPS
	Rx(Downlink): 1.57542GHz
	--



Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg)
Limit is 2.0(W/kg) for 10-g
	10-g Head
	1.360W/kg

	
	10-g Body
	1.004W/kg

	Limit is 4.0(W/kg) for 10-g
	10-g Member DAS
	2.415W/kg





Technical file held by: Shenzhen Doke Electronic Co., LTD
Address: 801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District,
Shenzhen, China

Signed for and on behalf of:                    Shenzhen Doke Electronic Co., Ltd
	Name and Title: 
	 zhang.liuwei /Manager

	Address: 
	801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China.



[image: C:\Users\ntek136\AppData\Roaming\DingTalk\34210522_v2\ImageFiles\ed\lQLPDhsGuRYAGLFlzPqw_071EMltR5QB27AqmEBCAA_250_101.png]
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(Name of product, type or model, batch or serial number)


 


 


System components:


 


PIFA Antenna


:BT/Wi


-


Fi2.4G:


2.2


dBi; WIFI5G:


2


.7


dBi;


 


GSM900:


 


-


1.58


dBi/DCS1800:


 


0.76


dBi; WCDMABand


?


: 


1.12


dBi,Band


?


:


 


-


1.58


dBi;


 


LTE: 


Band 1: 1.12dBi; Band 3: 0.76dBi; Band 7: 1.61dBi; Band 8: 


-


1.58dBi; Band 20: 


-


1.57dBi; 


 


Band 28: 


-


1.93dBi; Band 40: 1.46dBi; Band 41: 1.54dBi 


 


NR: 


N1: 1.12dBi; N3: 0.76dBi; N8: 


-


1.58dBi; N20: 


-


1.57dBi; N28: 


-


1.93dBi; 


 


N40: 1.46dBi; N41: 1.54dBi; N77: 2.21


dBi;N78: 2.23dBi


 


Adapter 


:


 


Model: QZ


-


04501EC00


 


Input: 100


-


240V~50/60Hz 1.2A


 


Output: 5.0V 3.0A 15.0W or 9.0V 3.0A 27.0W


 


     


or 12.0V 2.5A 30.0W or 15.0V 2.0A 30.0W


 


     


or 20.0V 2.25A 45.0W Max


 


(PPS) 5.0V


-


11.0V 3.0A 33.0W Max


 


(PPS) 5.0V


-


20.0V 2.25A 45.0W 


Max


 


Manufacturer:


 


Guangdong Quanzhi Technology Co., Ltd


 


 


RechargeableLi


-


ionBattery:


 


Model:


Li


386284HTT


;


 


Specification:DC 


3.8


7


V, 


75


0


0mAh,


29.025


Wh;


 


Manufacturer: 


Shenzhen Huatiantong Technology Co., Ltd


 


 


Hardware Version


:


 


F216_MAIN_PCB_V1.0


 


Software Version:


 


BL7000_NEU_F216_V1.0/PILOT 3_NEU_F216_V1.0/


 


BL7000 Pro_NEU_F216_V1.0


 




  Decl a r ation   of   C o nfo r m i t y   (DoC)     W e ,   Shen z hen   Do k e   El e c tro ni c   Co.,   L T D   801, B u il d in g 3, 7 t h I n du s t r ial   Z one,  Y ulv   Co m m un i t y ,  Y utang   Road,  G u a ng m ing  D i s t r i c t,   S h en z hen,  C h ina     Dec l a re   t hat   t he   D oC   is   i ss u e d   u nder   o ur   s ole   res pon s i b ili t y   a nd   b e l o ngs   t o   t he   f o ll o w ing   p r o d u c t(s) :    

Pr o duct   T y pe:  Smart  P hone    

T r a dem a r k ：    Blackview / OSCAL  

Model   N u mbe r(s ) :  BL7000,   PILOT 3, BL7000 Pro  

    (Na m e   o f   produ c t ,   t y p e   o r   m od e l,   b a tch   o r   s er ial   n u m ber )     (Name of product, type or model, batch or serial number)     System components:   PIFA Antenna :BT/Wi - Fi2.4G: 2.2 dBi; WIFI5G: 2 .7 dBi;   GSM900:   - 1.58 dBi/DCS1800:   0.76 dBi; WCDMABand ? :  1.12 dBi,Band ? :   - 1.58 dBi;   LTE:  Band 1: 1.12dBi; Band 3: 0.76dBi; Band 7: 1.61dBi; Band 8:  - 1.58dBi; Band 20:  - 1.57dBi;    Band 28:  - 1.93dBi; Band 40: 1.46dBi; Band 41: 1.54dBi    NR:  N1: 1.12dBi; N3: 0.76dBi; N8:  - 1.58dBi; N20:  - 1.57dBi; N28:  - 1.93dBi;    N40: 1.46dBi; N41: 1.54dBi; N77: 2.21 dBi;N78: 2.23dBi   Adapter  :   Model: QZ - 04501EC00   Input: 100 - 240V~50/60Hz 1.2A   Output: 5.0V 3.0A 15.0W or 9.0V 3.0A 27.0W         or 12.0V 2.5A 30.0W or 15.0V 2.0A 30.0W         or 20.0V 2.25A 45.0W Max   (PPS) 5.0V - 11.0V 3.0A 33.0W Max   (PPS) 5.0V - 20.0V 2.25A 45.0W  Max   Manufacturer:   Guangdong Quanzhi Technology Co., Ltd     RechargeableLi - ionBattery:   Model: Li 386284HTT ;   Specification:DC  3.8 7 V,  75 0 0mAh, 29.025 Wh;   Manufacturer:  Shenzhen Huatiantong Technology Co., Ltd     Hardware Version :   F216_MAIN_PCB_V1.0   Software Version:   BL7000_NEU_F216_V1.0/PILOT 3_NEU_F216_V1.0/   BL7000 Pro_NEU_F216_V1.0  

