
Declaration of Conformity (DoC)


We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Smart Phone

	Trademark：
	Blackview

	Model Number(s):
	FORT 5



Operating system:

Hardware Version: E5J7_MAIN_PCB_V1.1

Software Version: FORT_5_EEA_E5J7_V1.0_A16_01_20250107V02

(Name of product, type or model, batch or serial number)


System components:

NFC/WPT: Coil Antenna
PIFA Antenna
Bluetooth: 1.5dBi
2.4G WLAN: 1.5dBi
5G WLAN: 1.9dBi
GSM 900: -1.8 dBi; GSM 1800: 1.1 dBi
WCDMA B1: 1.2 dBi; WCDMA B8: -1.8 dBi
LTE B1: 1.2 dBi; LTE B3: 1.1 dBi; LTE B7: 1.2 dBi; LTE B8: -1.8 dBi; LTE B20: -1.9 dBi; LTE B28: -2.1 dBi

Adapter:
Model:  HJ-C6-33-EU  
Input: 100-240~50/60Hz 0.8A
Output: 5.0V 3.0A 15.0W or 9.0V 3.0A 27.0W or 12.0V 2.5A 30.0W or 15.0V 2.0A 30.0W or 20.0V 1.5A 30.0W 
PPS: 3.3V-11.0V 3.0A 33.0W MAX
Manufacturer: Shenzhen Huajin Electronics Co., Ltd

Rechargeable Li-ion Battery:
Model: LiFHPS496487PFH; Specification: DC 3.87V, 5000mAh 
Manufacturer: Guangdong Fenghua New Energy Co., Ltd.
USB Cable: 100cm;

[image: ]
The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

HEALTH & SAFETY (Art. 3(1)(a)):

EN 50360:2017+A1:2023 EN 50566:2017+A1:2023 EN IEC/IEEE 62209-1528:2021 EN 50663:2017 EN 62479:2010 
EN  IEC 62368-1:2020+A11:2020
EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11) 

ETSI EN 301 489-3 V2.3.2 (2023-01)

ETSI EN 301 489-17 V3.3.1 (2024-09)

ETSI EN 301 489-19 V2.2.1 (2022-09)

ETSI EN 301 489-52 V1.3.1 (2024-11) 

EN 55032:2015+A11:2020

EN IEC 61000-3-2:2019+A2:2024

EN 61000-3-3:2013+A2:2021+AC:2022

EN 55035:2017+A11:2020

Radio Spectrum (Article 3.2):
ETSI EN 300 328 V2.2.2 (2019-07)

ETSI EN 301 893 V2.1.1 (2017-05)

ETSI EN 300 440 V2.2.1 (2018-07)

EN300 330 V2.1.1(2017-02)

ETSI EN 303 345-1V1.1.1(2019-06)

ETSI EN 303 345-3V1.1.1(2021-06)

ETSI EN 303 413 V1.2.1 (2021-04)

ETSI EN 303 417 V1.1.1 (2017-09)

ETSI EN 301 511 V12.5.1 (2017-03)

ETSI TS 151 010-1 V13.14.0(2024-06)

ETSI EN 301 908-1 V15.2.1 (2023-01)

ETSI EN 301 908-2 V13.1.1 (2020-06)

ETSI EN 301 908-13 V13.3.1 (2024-10)


The submitted samples of the above equipment has been tested and found to comply with the following European Directives:
RoHS Directive 2011/65/EU & (EU) 2015/863






[bookmark: Notified_Body_Involved:]Notified Body Involved:


Notified Body Name: DERYCOM CERTIFICATION SERVICES, INC.
Notified Body Number: 3052
[bookmark: _GoBack]Notified Body Assessment Performed: Module B/C on Article 3.1a, 3.1b, 3.2 EU-type examination certificate number: JEC-66






















[bookmark: _Hlk218100528]RF Specification:

	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	3.24dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	1.38dBm

	WIFI 2.4G
802.11b/n(20MHz):
802.11n(40MHz):
	802.11b/n(20MHz):2412-2472MHz
802.11n(40MHz):2422~2462MHz
	14.01dBm

	[bookmark: OLE_LINK14]Wi-Fi 5.2G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac(80MHz):
	802.11a/n/ac (20MHz):5180~5240MHZ
802.11n/ac(40MHz):5190~5230MHZ
802.11ac(80MHz):5210MHz
	14.17dBm

	Wi-Fi 5.8G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac (80MHz):
	
802.11a/n/ac(20MHz):5745~5825MHz
802.11n /ac(40MHz):5755~5795MHz
802.11ac (80MHz):5775MHz
	13.53dBm

	GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;
RX(Downlink):925M‐960MHZ
	32.82dBm

	GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;
RX(Downlink):1805M‐1880MHZ
	29.70dBm

	WCDMA B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	23.10dBm

	WCDMA B8
	TX(Uplink): 880-915MHz;
RX(Downlink):925-960MHz
	22.64dBm

	LTE FDD B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	23.58dBm

	LTE FDD B3
	TX(Uplink) :1710-1785MHz;
RX(Downlink):1805-1880MHz
	23.36dBm

	LTE FDD B7
	TX(Uplink) :2500-2570MHz;
RX(Downlink):2620-2690MHz
	23.07dBm

	LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz
RX(Downlink): 925 MHz to 960 MHz
	23.17dBm

	LTE FDD B20
	TX(Uplink): 832MHz~862MHz;
RX(Downlink):791MHz~821MHz
	23.18dBm

	LTE FDD B28
	TX(Uplink):    703 MHz to 748MHz
RX(Downlink): 758 MHz to 803 MHz
	23.28dBm

	GPS (RX)
	Rx(Downlink): 1.57542GHz
	--

	NFC (RX)
	13.56MHZ
	--

	[bookmark: _Hlk218100437]WPT (RX)
	110.5kHz~205kHz
	--




Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet other body (at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	10-gHead
	0.147

	
	10-gBody
	1.498

	Limitis 4.0(W/kg) for10-g
	10-gMemberDAS
	1.498





Technical file held by: Shenzhen Doke Electronic Co., LTD

801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Signed for and on behalf of:                           Shenzhen Doke Electronic Co., LTD


	Name and Title:
	Liu yunlong/Manager

	Address:
	801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China




	

[image: ]
Signature of Authorized Person
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NFC/WPT:

Coil
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PIFA

Antenna

Bluetooth:

1.5dBi

2.4G
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5G

WLAN:
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3.3V-11.0V
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Co.,
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Li-ion
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Model:

LiFHPS496487PFH;

Specification:
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