
Declaration of Conformity (DoC)


We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Tablet PC

	Trademark：
	Blackview

	Model Number(s):
	MEGA 12



(Name of product, type or model, batch or serial number)


System components:For Bluetooth/2.4G WIFI/5G WIFI/GSM/WCDMA/
LTE/5G NR: PIFAAntenna 

 BT/Wi-Fi2.4G: -1.2dBi

WIFI 5.2G:0.6 dBi 

WIFI 5.8G:0.6 dBi
GSM900: 0.2 dBi, DCS1800: -0.8 dBi; WCDMA Band Ⅰ: -0.7 dBi ;Band Ⅷ:0.2 dBi;

LTE: Band 1: -0.7 dBi; Band 3: -0.8 dBi; Band 7: 1 dBi; Band 8: 0.2 dBi; Band 20: -0.2 dBi; Band 28: -1.8 dBi; 

NR: N1: -0.7 dBi, N3:-0.8 dBi, N8: 0.2 dBi, N20:-0.2 dBi, N28:-1.8 dBi, N40:0.4 dBi, N77:0.2 dBi, N78:0.3 dBi

GPS: PIFA Antenna 
NFC: Coil Antenna
FM: Earphone Antenna

Adapter:
Model:QZ-05500EC00
Input:100-240V~50/60Hz 1.2A
Output: 5.0V 2.0A or 5-20V 3-2.75A(MAX)
(PPS)5-20V 3-2.75A (MAX)
Manufacturer: Guangdong Quanzhi Technology Co.,Ltd.

Rechargeable Li-ion Battery:
Model: LiU3289113PHVUTL
Specification: DC 3.87V, 10000mAh 
Manufacturer: SHENZHEN UTILITY ENERGY CO., LTD.
USB Cable: 100cm;


The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

HEALTH & SAFETY (Art. 3(1)(a)):

EN 50566:2017+A1:2023   EN IEC/IEEE 62209-1528:2021    EN 50663:2017     EN 62479:2010 
EN 62368-1:2020+A11:2020
EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)

ETSI EN 301 489-3 V2.3.2 (2023-01)

ETSI EN 301 489-17 V3.3.1 (2024-09)

ETSI EN 301 489-19 V2.2.1 (2022-09)

ETSI EN 301 489-52 V1.3.1 (2024-11)

EN 55032:2015+A11:2020; EN 55035:2017+A11:2020

EN IEC 61000-3-2:2019+A2:2024; EN 61000-3-3:2013+A2:2021+AC:2022

Radio Spectrum (Article 3.2):

ETSI EN 301 511 V12.5.1 (2017-03)

ETSI TS 151 010-1 V13.14.0(2024-06)

ETSI EN 301 908-1 V15.2.1 (2023-01)

ETSI EN 301 908-2 V13.1.1 (2020-06)

ETSI EN 301 908-13 V13.3.1 (2024-10)

ETSI TS 138 521-1 V17.6.1 (2022-10)

ETSI TS 138 521-3 V17.7.0(2023-01)

ETSI EN 301 908-1 V15.2.1 (2023-01)

ETSI EN 301 908-25 V15.1.1 (2024-10)

ETSI EN 300 328 V2.2.2 (2019-07)

ETSI EN 301 893 V2.1.1 (2017-05)

ETSI EN 300 440 V2.2.1 (2018-07)

ETSI EN 303 345-1 V1.1.1 (2019-06)

ETSI EN 303 345-3 V1.1.1 (2021-06)

ETSI EN 303 413 V1.2.1 (2021-04)

ETSI EN 300 330 V2.1.1 (2017-02)










The submitted samples of the above equipment has been tested and found to comply with the following European Directives:
RoHS Directive 2011/65/EU & (EU) 2015/863











[bookmark: Notified_Body_Involved:]Notified Body Involved:


Notified Body Name: DERYCOM CERTIFICATION SERVICES, INC.
Notified Body Number: 3052
Notified Body Assessment Performed: Module B/C on Article 3.1a, 3.1b, 3.2 EU-type examination certificate number: JEC-53
























RF Specification:

	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	 2.73 dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	2.06 dBm

	WIFI 802.11b/g/

n(HT20/40)
	802.11b/g/n(20MHz): 2412~2472MHz;

802.11n(40MHz):2422~2462MHz
	
17.42dBm

	[bookmark: OLE_LINK14]Wi-Fi 5.2G(802.11a/n20/ac 20)
	
802.11a/ n20/ac 20:5180MHz~5240MHz

802.11 n40/ac 40:5190MHz~5230MHz

802.11 ac 80:5210MHz
	


15.14dBm

	Wi-Fi 5.8G(802.11a/n20/n40/ac 20/ac40/ac80
)
	
802.11a/ n20/ac 20:5745MHz~5825MHz

802.11 n40/ac 40:5755MHz~5795MHz

802.11 ac 80:57750MHz
	


13.36dBm

	
GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;

RX(Downlink):925M‐960MHZ
	
33.34dBm

	
GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;

RX(Downlink):1805M‐1880MHZ
	
30.04dBm

	
WCDMA B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
23.69dBm

	
WCDMA B8
	TX(Uplink): 880-915MHz;

RX(Downlink):925-960MHz
	
23.15 dBm

	
LTE FDD B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
21.59 dBm

	
LTE FDD B3
	TX(Uplink) :1710-1785MHz;

RX(Downlink):1805-1880MHz
	
22.22 dBm

	
LTE FDD B7
	TX(Uplink) :2500-2570MHz;

RX(Downlink):2620-2690MHz
	
21.11dBm

	
LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz

RX(Downlink): 925 MHz to 960 MHz
	
22.61dBm

	
LTE FDD B20
	TX(Uplink): 832MHz~862MHz;

RX(Downlink):791MHz~821MHz
	
22.09dBm

	
LTE FDD B28
	TX(Uplink): 703 MHz to 748MHz

RX(Downlink): 758 MHz to 803 MHz
	
 22.28 dBm

	5G NR: N1
	1920-1980 MHz (TX),
2110-2170 MHz (RX)
	
22.29 dBm

	5G NR: N3
	1710-1785 MHz (TX),
1805-1880 MHz (RX)
	
22.19dBm

	5G NR: N8
	880-915 MHz (TX), 
925-960 MHz (RX)
	
23.29dBm



	5G NR: N20
	832-862 MHz (TX), 
791-821 MHz (RX)
	
23.16dBm

	5G NR: N28
	703-748 MHz (TX), 
758-803 MHz (RX)
	
 22.99 dBm

	5G NR: N40
	2300-2400 MHz (TX), 
2300-2400 MHz (RX)
	22.81 dBm

	5G NR: N77
	3300-4200 MHz (TX), 
3300-4200 MHz (RX)
	24.1 dBm

	5G NR: N78
	3300-3800MHz(TX), 
3300-3800MHz(RX)
	24.26 dBm

	FM
	Rx(Downlink): 87.5MHz~108MHz
	--

	GPS
	Rx(Downlink): 1.57542GHz
	--

	NFC
	13.56 MHz(
	--






Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	[bookmark: _GoBack]10-g Body&Limbs
	1.901W/kg













Technical file held by: Shenzhen Doke Electronic Co., LTD
Address	：801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China
Signed for and on behalf of:                            Shenzhen Doke Electronic Co., LTD

	Name and Title:
	Liu yunlong/ Manager

	Address:
	801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China
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