
Declaration of Conformity (DoC)


We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Smart Phone

	Trademark：
	Blackview

	Model Number(s):
	ROCK 3



Operating system:

Hardware Version:E5J7_MAIN_PCB_V1.1

Software Version :/

(Name of product, type or model, batch or serial number)


System components:

PIFA Antenna: BT/Wi-Fi2.4G:1.23dBi; WIFI5G:0.89dBi

GSM 900:-4.16dBi, GSM 1800:-0.41dBi 
WCDMA B1 0.78dBi, WCDMA B8 -4.16 dBi 
LTE Band-1: 0.78dBi, LTE Band-3: -0.41dBi, LTE Band-7: 1.17dBi, LTE Band-8: -4.16dBi, LTE Band-20: -5.97dBi, LTE Band-28: -6.77dBi
NFC: 0dBi
GPS: PIFA Antenna 
WPT: Coil Antenna

Adapter:
Model: QZ-03301EC00 
Input: 100-240~50/60Hz 1.2A
Output: 5.0V 3.0A 15.0W 
or 9.0V 3.0A 27.0W 
or 12.0V 2.5A 30.0W 
or 15.0V 2.0A 30.0W 
or 20.0V 1.5A 30.0W Max
(PPS) 5.0V-11.0V 3.0A 33.0W Max
Manufacturer: Guangdong Quanzhi Technology Co., Ltd.
[bookmark: _GoBack]
Rechargeable Li-ion Battery:
Model: LiU536587P-HTT; Specification: DC 3.85V, 10000mAh 
Manufacturer: SHENZHEN HUATIANTONG TECHNOLOGY CO.LTD 
USB Cable: 100cm;

[image: ]
The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

HEALTH & SAFETY (Art. 3(1)(a)):

EN 50360:2017+A1:2023 EN 50566:2017+A1:2023 EN IEC/IEEE 62209-1528:2021 EN 50663:2017 EN 62479:2010 
EN  IEC 62368-1:2020+A11:2020
EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)

ETSI EN 301 489-3 V2.3.2 (2023-01)

ETSI EN 301 489-17 V3.3.1 (2024-09)

ETSI EN 301 489-19 V2.2.1 (2022-09)

ETSI EN 301 489-52 V1.3.1 (2024-11)

EN 55032:2015+A11:2020; EN 55035:2017+A11:2020

EN IEC 61000-3-2:2019+A2:2024; EN 61000-3-3:2013+A2:2021+AC:2022

Radio Spectrum (Article 3.2):

ETSI EN 301 511 V12.5.1 (2017-03);

ETSI EN 301 908-1 V15.2.1 (2023-01)

ETSI EN 301 908-2 V13.1.1 (2020-06)

ETSI EN 301 908-13 V13.3.1 (2024-10)

EN 300 328 V2.2.2 (2019-07);

EN 301 893 V2.1.1 (2017-05);

EN 300 440 V2.2.1 (2018-07);

EN300 330 V2.1.1 (2017-02)

EN 303 413 V1.2.1 (2021-04);

EN300 330 V2.1.1 (2017-02)

EN 303 417 V1.1.1 (2017-09)

EN 303 345-1 V1.1.1 (2019-06)

EN 303 345-3 V1.1.1 (2021-06)



The submitted samples of the above equipment has been tested and found to comply with the following European Directives:
RoHS Directive 2011/65/EU & (EU) 2015/863






[bookmark: Notified_Body_Involved:]Notified Body Involved:


Notified Body Name: DERYCOM CERTIFICATION SERVICES, INC.
Notified Body Number: 3052
Notified Body Assessment Performed: Module B/C on Article 3.1a, 3.1b, 3.2 EU-type examination certificate number: JEC-60























[bookmark: _Hlk218100528]RF Specification:

	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	3.12dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	4.32dBm

	WIFI 2.4G
802.11b/n(20MHz):
802.11n(40MHz):
	
802.11b/n(20MHz):2412-2472MHz
802.11n(40MHz):2422~2462MHz
	
14.1dBm

	[bookmark: OLE_LINK14]Wi-Fi 5.2G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac(80MHz):
	
802.11a/n/ac (20MHz):5180~5240MHZ
802.11n/ac(40MHz):5190~5230MHZ
802.11ac(80MHz):5210MHz
	


13.74dBm

	Wi-Fi 5.8G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac (80MHz):
	
802.11a/n/ac(20MHz):5745~5825MHz
802.11n /ac(40MHz):5755~5795MHz
802.11ac (80MHz):5775MHz
	


13.6dBm

	
GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;

RX(Downlink):925M‐960MHZ
	
33.04dBm

	
GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;

RX(Downlink):1805M‐1880MHZ
	
30.23dBm

	
WCDMA B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
24.67dBm

	
WCDMA B8
	TX(Uplink): 880-915MHz;

RX(Downlink):925-960MHz
	
23.93dBm

	
LTE FDD B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
23.37dBm

	
LTE FDD B3
	TX(Uplink) :1710-1785MHz;

RX(Downlink):1805-1880MHz
	
23.05 dBm

	
LTE FDD B7
	TX(Uplink) :2500-2570MHz;

RX(Downlink):2620-2690MHz
	
23.00dBm

	
LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz

RX(Downlink): 925 MHz to 960 MHz
	
22.91 dBm

	
LTE FDD B20
	TX(Uplink): 832MHz~862MHz;

RX(Downlink):791MHz~821MHz
	
23.05dBm

	
LTE FDD B28
	TX(Uplink):    703 MHz to 748MHz

RX(Downlink): 758 MHz to 803 MHz
	
23.18dBm

	GPS (RX)
	Rx(Downlink): 1.57542GHz
	

	NFC
	13.56MHZ
	-21.54 dBμA/m@10m

	[bookmark: _Hlk218100437]WPT (RX)
	110.5kHz~205kHz
	--




Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	10-gHead
	0.631

	
	10-gBody
	0.546

	Limitis 4.0(W/kg) for10-g
	10-gMemberDAS
	0.546





Technical file held by: Shenzhen Doke Electronic Co., LTD

801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Signed for and on behalf of:                           Shenzhen Doke Electronic Co., LTD


	Name and Title:
	Zhang liuwei/Manager

	Address:
	801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China
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