
Declaration of Conformity (DoC)


[bookmark: We,_Shenzhen_Doke_Electronic_Co.,_LTD]We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Smart Phone

	
Trademark：  
	Blackview

	Model Number(s):
	ROCK 5, BV9300Pro Plus

	Hardware Version:
	E5J7_MAIN_PCB_V1.1

	Software Version:
	N/A

	Operating system:
	Android






(Name of product, type or model, batch or serial number)


System components:

PIFA Antenna; gain: BT/Wi-Fi2.4G: 1.45dBi; WIFI5G:1.09dBi; GSM900:-4.21dBi/DCS1800:0.17dBi
WCDMA:Band Ⅰ:0.84dBi ;Band Ⅷ:-4.58dBi;

LTE: Band 1: 0.89dBi; Band 3: 0.18dBi; Band 7:1.37dBi; Band 8: -4.24dBi; Band 20: -5.85dBi; Band 28: -6.54dBi; GPS: PIFA Antenna; NFC: Coil Antenna
FM: Use earphone as Antenna



Adapter:
Model: QZ-03301EC00
Brand: Blackview
Input: 100-240~50/60Hz 1.2A
Output: 5.0V 3.0A 15.0W or 9.0V 3.0A 27.0W or 12.0V 2.5A 30.0W or 15.0V 2.0A 30.0W or 20.0V 1.5A 30.0W Max
PPS: 5.0V-11.0V 3.0A 33.0W Max
Manufacturer: Guangdong Quanzhi Technology Co.,Ltd. Rechargeable Li-ion Battery:
Model: U476591PNJ; Specification: DC 3.85V, 5000mAh,19.25Wh
Manufacturer: Guangdong Quanzhi Technology Co.,Ltd

USB Cable: 110cm;


[image: ]

The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

[bookmark: HEALTH_&_SAFETY_(Art._3(1)(a)):]HEALTH & SAFETY (Art. 3(1)(a)):

EN IEC 62368-1:2020+A11:2020
EN 50360: 2017+A1:2023; 
EN 50566: 2017+A1:2023
EN IEC/IEEE 62209-1528: 2021
EN 50663: 2017; EN 62479: 2010

EMC (Art. 3(1)(b)):
EN 301 489-1 V2.2.3 (2019-11)
EN 301 489-3 V2.3.2 (2023-01)
EN 301 489-17 V3.3.1(2024-09)
EN 301 489-19 V2.2.1 (2022-09)
EN 301 489-52 V1.3.1 (2024-11)
EN 55032:2015+A11:2020
EN IEC 61000-3-2:2019+A2:2024
EN 61000-3-3:2013+A2:2021+AC:2022
EN 55035:2017+A11:2020
[bookmark: Radio_Spectrum_(Article_3.2):]Radio Spectrum (Article 3.2):
EN 301 511 V12.5.1 (2017-03)  
TS 151 010-1 V13.14.0 (2024-06)
EN 301 908-1 V15.2.1 (2023-01)
EN 301 908-2 V13.1.1 (2020-06)
EN 301 908-13 V13.3.1 (2024-10)
EN 300 328 V2.2.2 (2019-07)
EN 301 893 V2.1.1 (2017-05)
EN 300 440 V2.2.1 (2018-07)
EN 303 345-1 V1.1.1 (2019-06)
EN 303 345-3 V1.1.1 (2021-06)
EN 303 413 V1.2.1 (2021-04)
EN300 330 V2.1.1 (2017-02)
The submitted samples of the above equipment has been tested and found to comply with the following European 
Directives: RoHS Directive 2011/65/EU & (EU) 2015/863

NOTIFIEDBODY:
[bookmark: Name:DERYCOM_CERTIFICATION_SERVICES,_INC]Name: LGAl Technological Center S.A. (APPLUS)

Address: Campus UAB. Ronda de la Font del Carme s/n08193 Bellaterra, Barcelona (Spain)

IdentificationNumber: 0370

EU-type examination certificate number: No. 0370-RED-11439
 

[bookmark: RF_Specification:]RF Specification:

	[bookmark: _Hlk229239257]Function
	Operation Frequency
	Max RF output power:

	BLE 1M
	2402MHz–2480MHz
	3.95 dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	3.65 dBm 

	WIFI 802.11b/g/
n(HT20/40)
	802.11b/g/n(20MHz): 2412~2472MHz;
802.11n(40MHz):2422~2462MHz
	13.95dBm 

	Wi-Fi
5.2G(802.11a/n20/n40/ac2
0/ac40/ac80)
	802.11a/ n20/ac20:5180MHz~5240MHz
802.11 n40/ac40:5190MHz~5230MHz
802.11 ac80:5210MHz
	
13.58 dBm 

	Wi-Fi
5.8G(802.11a/n20/n40/ac2
0/ac40/ac80)
	802.11a/ n20/ac20:5745MHz~5825MHz
802.11 n40/ac40:5755MHz~5795MHz
802.11 ac80:57750MHz
	
11.60 dBm 

	GSM/GPRS/EGPRS 900
	TX(Uplink):880M-915MHZ;
RX(Downlink):925M-960MHZ
	32.84 dBm 

	GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M-1785MHZ;
RX(Downlink):1805M-1880MHZ
	29.94 dBm  

	WCDMA B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	22.86 dBm  

	WCDMA B8
	TX(Uplink): 880-915MHz;
RX(Downlink):925-960MHz
	23.84 dBm  

	LTE FDD B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	23.37dBm

	LTE FDD B3
	TX(Uplink) :1710-1785MHz;
RX(Downlink):1805-1880MHz
	22.65 dBm

	LTE FDD B7
	TX(Uplink) :2500-2570MHz;
RX(Downlink):2620-2690MHz
	22.56 dBm

	LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz
RX(Downlink): 925 MHz to 960 MHz
	22.94 dBm

	LTE FDD B20
	TX(Uplink): 832MHz~862MHz;
RX(Downlink):791MHz~821MHz
	23.11 dBm

	LTE FDD B28
	TX(Uplink): 703-748 MHz (TX), 
RX(Downlink): 758-803 MHz
	22.98dBm

	FM
	Rx(Downlink): 87.5MHz~108MHz
	--

	GPS
	Rx(Downlink): 1.57542GHz
	--

	NFC
	13.56 MHz
	-40.46dBm



Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 0mm) are:

	Max SAR Value(W/kg) Limitis 2.0(W/kg) for10-g
	
Head
	
0.785 W/kg

	
	
Body
	
0.534W/kg

	Max SAR Value(W/kg) Limitis 4.0(W/kg) for10-g
	 Member DAS
	0.534W/kg





[bookmark: _Hlk229240171]Technical file held by: Shenzhen Doke Electronic Co., LTD
Address: 801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Signed for and on behalf of:	Shenzhen Doke Electronic Co., LTD

	Name and Title:
	[bookmark: _Hlk229240150]Hong zongqing/ Manager

	Address:
	
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China





[image: ]

[bookmark: Signature_of_Authorized_Person]Signature of Authorized Person
[bookmark: _GoBack]2026.5.6
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  Decla r a t i o n   o f   C o n f o r m i t y   ( D o C)       W e ,   S h en z hen   D o k e   E l e c tr on i c  C o.,   L T D   801, B u il di n g 3,   7 t h   I n du s t r i al   Z one,  Y ulv   C o m m u n i t y ,  Y uta n g   R oad,  G u a ng m ing   D i s t r i c t,   S h en z hen,  C h ina     Dec l ar e   t h a t   t he   D oC   is   i s s u e d   u nd e r   o ur   s ole   r es p o n s i b i l i t y   a nd   b e l o ngs   t o   t he   f o l l o w ing   p rod u c t (s ) :    

P r od u c t   T y p e:  S ma rt   P hon e  

  T ra d e m a r k ：      Blackview  

Mod e l   N u m b e r(s ) :  ROCK 5 ,  BV9300Pro Plus  

Hardware Version :  E5J7_MAIN_PCB_V1.1  

Software Version:  N/A  

O perating system :  Android  

        (N a m e   o f   pr o du c t ,   t y p e   o r   m od e l,   b a t c h   o r   s e r i a l   n u m b er )       S y s t e m   c o m p o ne n ts :     P I F A   A n t e nn a ;   ga i n :   B T / W i - F i 2.4 G :   1.45 d B i ;   W I F I5 G : 1.09 d B i ;  G S M 90 0 : - 4.21 d B i/ D C S 1 80 0 : 0.17 d B i   W C D M A : B an d   Ⅰ : 0 . 8 4 d B i   ; B an d   Ⅷ : - 4.58 d B i ;     L T E :   B an d   1 :   0.89 d B i ;   B an d   3 :   0.18 d B i ;   B a n d   7 : 1.37 d B i ;   B an d   8 :   - 4.24 d B i ;   B an d   2 0 :   - 5.85 d B i ;  B an d   2 8 :   - 6.54 d B i ;  G P S :   PI F A   A n t enn a;  NFC :   Coil   A n t enn a   F M :   U s e   earph o n e   a s   A n t enna         A d a p t e r :   Model: QZ - 03301EC00   Brand: Blackview   Input: 100 - 240~50/60Hz 1.2A   Output: 5.0V  3.0A 15.0W or 9.0V 3.0A 27.0W or 12.0V 2.5A 30.0W or 15.0V 2.0A 30.0W or 20.0V 1.5A 30.0W Max   PPS: 5.0V - 11.0V 3.0A 33.0W Max   M anu f a c t ure r :   Gu a ng d on g   Qu a n z h i   T e c h no l o g y  C o ., L t d .   R e c ha r ge a b le   L i - i o n   B a tt e r y :   M ode l:   U 4 76 5 9 1 P N J ;   S p e c i f i c a ti o n :   D C   3 . 8 5 V,   5 00 0 mA h , 19 . 2 5 W h   M anu f a c t ure r :   Guangdong Quanzhi Technology Co.,Ltd     U SB   Cab l e :   1 1 0 c m;      

