
Declaration of Conformity (DoC)


We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Smart Phone

	Trademark：  
	Blackview

	Model Number(s):
	WAVE 7C

	Hardware Version:
	J567F_610_310_D4EF_V1.0

	Operating system:
	Android 





(Name of product, type or model, batch or serial number)


System components:

PIFA Antenna; gain: BT/Wi-Fi2.4G:6.6dBi;WIFI5G:0.82dBi; GSM900:-2.08 dBi/DCS1800:-2.4dBi
WCDMA:Band Ⅰ:0.88dBi ;Band Ⅷ:-2.08dBi;

LTE: Band 1: 0.88dBi; Band 3: -2.4dBi; Band 7:2.1dBi; Band 8: -2.08dBi; Band 20: -4.39dBi; GPS: PIFA Antenna
FM: Use earphone as Antenna



Adapter:
Model: QZ-01004EA00
Input: 100-240V~50/60Hz 0.3A
Output:       5.0V2.0A, 10.0W
Manufacturer: Guangdong Quanzhi Technology Co.,Ltd. Rechargeable Li-ion Battery:
Model: U476591PNJ; Specification: DC 3.85V, 5000mAh,19.25Wh Manufacturer: Shenzhen Nuojia Technology Industrial Co.,LTD

USB Cable: 110cm;




The object of the declaration described above is in conformity with the essential requirements of

the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU). The following harmonized standards and technical specifications have been applied: HEALTH & SAFETY (Art. 3(1)(a)):
EN 50360:2017;
EN 50360:2017/A1:2023 EN 50566:2017;
EN 50566:2017/A1:2023
EN IEC/IEEE 62209-1528:2021
EN 62479:2010
EN IEC 62368-1:2020+A11:2020
EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)
ETSI EN 301 489-3 V2.3.2 (2023-01)
ETSI EN 301 489-17 V3.3.1 (2024-09)
ETSI EN 301 489-19 V2.2.1 (2022-09)
ETSI EN 301 489-52 V1.2.1 (2021-11) EN 55032:2015+A1:2020
EN 55035:2017+A11:2020
EN IEC 61000-3-2:2019+A1:2021 EN 61000-3-3:2013+A2:2021

Radio Spectrum (Article 3.2):

ETSI EN 301 511 V12.5.1 (2017-03);
ETSI EN 301 908-1 V15.2.1 (2023-01)
ETSI EN 301 908-2 V13.1.1 (2020-06);
ETSI EN 301 908-13 V13.2.1 (2022-02)
ETSI EN 300 328 V2.2.2 (2019-07);
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 300 440 V2.2.1 (2018-07)
ETSI EN 303 413 V1.2.1 (2021-04) ;
ETSI EN 303 345-1 V1.1.1 (2019-06);
ETSI EN 303 345-3 V1.1.1 (2021-06)


NOTIFIEDBODY:
Name:DERYCOM CERTIFICATION SERVICES, INC.
Address:1100 FalconAvenueGlencoe,Mn55336 Notified Body ID number: 3052
Certificate Number: JEC-71

RF Specification:

	Function
	Operation Frequency
	Max RF output power:

	BLE 1M
	2402MHz–2480MHz
	7.87 dBm

	BLE 2M
	2402MHz–2480MHz
	7.78 dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	8.64 dBm 

	WIFI 802.11b/g/
n(HT20/40)
	802.11b/g/n(20MHz): 2412~2472MHz;
802.11n(40MHz):2422~2462MHz
	16.28dBm 

	Wi-Fi
5.2G(802.11a/n20/n40/ac2
0/ac40/ac80)
	802.11a/ n20/ac20:5180MHz~5240MHz
802.11 n40/ac40:5190MHz~5230MHz
802.11 ac80:5210MHz
	
11.84 dBm 

	Wi-Fi
5.8G(802.11a/n20/n40/ac2
0/ac40/ac80)
	802.11a/ n20/ac20:5745MHz~5825MHz
802.11 n40/ac40:5755MHz~5795MHz
802.11 ac80:57750MHz
	
12.34 dBm 

	GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;
RX(Downlink):925M‐960MHZ
	31.96 dBm 

	GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;
RX(Downlink):1805M‐1880MHZ
	30.14 dBm  

	WCDMA B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	22.49 dBm  

	WCDMA B8
	TX(Uplink): 880-915MHz;
RX(Downlink):925-960MHz
	22.86 dBm  

	LTE FDD B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	23.45dBm

	LTE FDD B3
	TX(Uplink) :1710-1785MHz;
RX(Downlink):1805-1880MHz
	23.72 dBm

	LTE FDD B7
	TX(Uplink) :2500-2570MHz;
RX(Downlink):2620-2690MHz
	23.58 dBm

	LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz
RX(Downlink): 925 MHz to 960 MHz
	23.37 dBm

	LTE FDD B20
	TX(Uplink): 832MHz~862MHz;
RX(Downlink):791MHz~821MHz
	22.89 dBm

	FM
	Rx(Downlink): 87.5MHz~108MHz
	--

	GPS
	Rx(Downlink): 1.57542GHz
	--



Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg) Limitis 2.0(W/kg) for10-g
	
[bookmark: _GoBack]Head
	
0.344 W/kg

	
	
Body
	
1.112W/kg

	Max SAR Value(W/kg) Limitis 4.0(W/kg) for10-g
	 Member DAS
	2.060W/kg





Technical file held by: Shenzhen Doke Electronic Co., LTD
Address: 801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Signed for and on behalf of:	Shenzhen Doke Electronic Co., LTD

	Name and Title:
	Xie ce / Manager

	Address:
	
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China







Signature of Authorized Person
2026-1-29
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  Decl a r ation   o f   C o nfo r m i t y   (DoC)       W e ,   S h en z hen   D o k e   E l e c tr on i c Co.,   L T D   801, B u il di n g 3,   7 t h  I n du s t r i al   Z one,   Y ulv   C o m m u n i t y ,  Y uta n g   Road,   G u a ng m ing   D i s t r i c t,   S h en z hen, C hi na     Dec l ar e   t hat   t he   D oC   is   i s s u e d   u nder   o ur   s ole   r es p o n s i b i l i t y   a nd   b e l o ngs   t o   t he   f o l l o w ing   p rod u c t (s ) :    

P r od uct   T y pe:  Sm art   P h o ne  

T ra dem a r k ：      Bl a ck v i ew  

Model   N u mb e r (s ) :  WA V E  7 C  

Hardware Version :  J 567 F_ 6 10_310_D4 EF_V1.0  

O perating system :  Android   

      (N a m e   o f   pr o du c t ,   t y p e   o r   m od e l,   b a tch   o r   s e r ial   n u m b er )       S y s t e m   c o m p o ne n ts:     P I F A   A n t e nn a ;   ga i n :   B T / W i - F i 2.4 G :6 . 6 d B i ; W I F I5 G : 0 . 82 d B i ;  G S M 90 0 : - 2 . 0 8   d B i / D C S 1 80 0 : - 2 . 4 d B i   W C D M A : B an d   Ⅰ : 0 . 88 d B i   ; B an d   Ⅷ : - 2 . 0 8 d B i ;     L T E :   B an d   1 :   0 .88 d B i ;   B an d   3 :   - 2 . 4 d B i ;   B an d   7 : 2 . 1 d B i ;   B an d   8 :   - 2 . 0 8 d B i ;   B an d   2 0 :   - 4.39 d B i ;  G P S :   P I F A   A n t enn a   F M :   U s e   earph o n e   a s   A n t enn a         A d a p t e r :   M ode l :   Q Z - 0 1 00 4 EA 0 0   I n p u t :   1 0 0 - 2 40 V ~ 5 0 / 6 0 H z   0 . 3 A   O u t p u t :         5 . 0 V 2 . 0 A ,   10 . 0 W   M anu f a c t ure r :   Gu a ng d o ng   Qu a n z h i   Tec h no l o g y   C o . , L t d .  Re c har g e a b le  L i - ion B a tt e r y :   M ode l:   U 4 76 5 9 1 P N J ;   S p e c i f i c a ti o n :   D C   3 . 8 5 V,   5 00 0 mA h , 19 . 2 5 W h  M anu f a c t ure r :   S hen z he n  Nuo jia  T e c hno lo g y   I ndu s t r ial   C o ., L TD     U SB   Cab le :   1 1 0 c m;      

