EU Declaration of Conformity (DoC)

	Company name
	[bookmark: OLE_LINK24]HONG KONG LELEGAO TECHNOLOGY CO.,LIMITED

	Postal address
	19H Maxgrand Plaza, No.3 Tai Yau Street, San Po Kong, Kowloon, HongKong

	Postcode and City
	HongKong

	Telephone number
	+86 75532909320

	E-mail address
	zxy@blackview.hk


We declare that the DoC is issued under our sole responsibility and belongs to the following product:
	Equipment manufacturer
	Shenzhen Doke Electronic Co., LTD

	Type
	[bookmark: OLE_LINK31][bookmark: OLE_LINK32]XPLORE 6, XPLORE 6 Pro

	Product description
	Rugged Smartphone

	HW version
	G2596-MS-V3.0
	SW version
	XPLORE6_EEA_G2596_V1.0_A16 

	Optional accessories or System components
	Battery 
Model: Li536385HTT  
Rated Voltage: 7.6V
Charge Limit Voltage: 9.06V
Capacity: 6000mAh

Adapter 
Model: HJPD120-EU  
Brand: Blackview 
Input: 100-240V 50/60Hz 3.0A Max.  
Output: USB-C:5.0V 3.0A(15.0W)or 9.0V 3.0A(27.0W) or 
12.0V 3.0A(36.0W)or 15.0V 3.0A(45.0W) or 20.0V 6.0A(120.0W) (PPS)5.0V 20.0V 6.0A(120.0W Max)
Output USB-A: 5.0V 3.0A(15.0W) or 9.0V 3.0A(27.0W)or 
12.0V 3.0A(36.0W)or 15.0V 3.0A(45.0W) or 20.0V 3.0A(60.0W) 
(PPS)5.0V-20.0V 3.0A(60.0W Max)



The object of the declaration described above is in conformity with the relevant Union Harmonisation Legislation:
	RE Directive 2014/53/EU
	



The Notified Body Name: LGAI Technological Center S.A./Applus (Nr. 0370), has conducted the conformity assessment according to module B of Directive 2014/53/EU (RED) and issues the EU type certificate [0370-RED-12025].

The following standards and technical specifications have been applied for RE Directive 2014/53/EU:

	[bookmark: _Hlk233362588]Article 3.1a: Safety and Health
	EN IEC 62368-1:2020+A11:2020 
EN 50360: 2017/A1:2023
EN 50566: 2017/A1:2023
EN IEC/IEEE 62209-1528:2021
EN 50663: 2017; EN 62479: 2010

	Article 3.1b: EMC
	ETSI EN 301 489-1 V2.2.3 (2019-11) 
ETSI EN 301 489-3 V2.3.2 (2023-01)
ETSI EN 301 489-17 V3.3.1 (2024-09) 
ETSI EN 301 489-19 V2.2.1 (2022-09) 
ETSI EN 301 489-52 V1.3.1 (2024-11)
EN 55032:2015+A11:2020
EN IEC 61000-3-2:2019+A2:2024
EN 61000-3-3:2013+A2:2021+AC:2022
EN 55035:2017+A11:2020

	Article 3.2: RF Spectrum Efficiency
	ETSI EN 301 511 V12.5.1 (2017-03)  
ETSI TS 151 010-1 V13.14.0 (2024-06)
ETSI EN 301 908-1 V15.2.1 (2023-01)
ETSI EN 301 908-2 V13.1.1 (2020-06)
ETSI EN 301 908-13 V13.3.1 (2024-10)
ETSI TS 138 521-1 V17.6.1 (2022-10)
ETSI TS 138 521-3  V17.7.0 (2023-01)
ETSI EN 301 908-25 V15.1.1 (2024-10)
ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 300 440 V2.2.1 (2018-07)
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 303 413 V1.2.1 (2021-04)
ETSI EN 300 330 V2.1.1 (2017-02)
ETSI EN 303 345-1 V1.1.1 (2019-06)
ETSI EN 303 345-3 V1.1.1 (2021-06)

	Article 3.3: Special requirements invoked
	Not applicable




The following standards and technical specifications have been applied for the other European Legislation:
	
	







Operating Bands (Tx and Rx) and max power issued per TX band
BLE (Support 1M PHY, 2M PHY) 2402MHz–2480MHz 4.04dBm
BT(BR+EDR) 2402MHz–2480MHz 3.97dBm
2.4G WIFI 802.11b/g/n(20MHz): 2412~2472MHz 16.77dBm
5.2G WIFI:
802.11a/n/ac (20MHz): 5180~5240MHz
802.11n /ac (40MHz):5190~5230MHz
802.11ac (80MHz):5210MHz	16.12dBm
5.8G WLAN:
802.11a/n/ac (20MHz): 5745~5825MHz
802.11n /ac (40MHz):5755~5795MHz
802.11ac (80MHz):5775MHz    13.29dBm
GSM:
GSM 900: 880 ~ 915 MHz(TX), 925 ~ 960 MHz (RX) 33.01dBm
GSM 1800:1710 ~ 1785 MHz(TX), 1805 ~ 1880 MHz(RX) 29.29dBm
WCDMA:
WCDMA B1:1920-1980 MHz(TX), 2110-2170 MHz(RX) 24.18dBm
WCDMA B8:880-915 MHz(TX), 925-960 MHz(RX)    23.22dBm
LTE:
FDD LTE Band 1: 1920-1980 MHz (TX), 2110-2170 MHz (RX) 24.14dBm
FDD LTE Band 3: 1710-1785 MHz (TX), 1805-1880 MHz (RX) 23.49dB
FDD LTE Band 7: 2500-2570 MHz (TX), 2620-2690 MHz (RX) 23.77dBm
FDD LTE Band 8: 880-915 MHz (TX), 925-960 MHz (RX) 23.31dBm
FDD LTE Band 20: 832-862 MHz (TX), 791-821 MHz (RX) 23.23dBm
FDD LTE Band 28: 703-748 MHz (TX), 758-803 MHz (RX) 23.34dBm
5G NR:
N1: 1920-1980 MHz (TX), 2110-2170 MHz (RX) 21.96dBm 
N3: 1710-1785 MHz (TX), 1805-1880 MHz (RX) 23.16dBm 
N8: 880-915 MHz (TX), 925-960 MHz (RX) 23.75dBm
N20: 832-862 MHz (TX), 791-821 MHz (RX) 23.43dBm  
N28: 703-748 MHz (TX), 758-803 MHz (RX)  23.79dBm 
N40: 2300-2400 MHz (TX), 2300-2400 MHz (RX) 23.09dBm 
N77: 3300-4200 MHz(TX), 3300-4200 MHz(RX) 23.38dBm 
N78: 3300-3800MHz(TX), 3300-3800MHz(RX) 23.26dBm
[bookmark: _GoBack]GPS(RX):1575.42MHz FM: 87.5-108MHz
NFC 13.56 MHz  -21.36dBμA/m@10m
Tests for SAR are conducted using standard operating positions with the device transmitting at its highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:
	Max SAR Value(W/kg) Limitis 2.0(W/kg) for10-g
	
Head
	
1.096 W/kg

	
	
Body
	
1.656 W/kg

	Max SAR Value(W/kg) Limitis 4.0(W/kg) for10-g
	 Member DAS
	1.656 W/kg



Signed on behalf of: HONG KONG LELEGAO TECHNOLOGY CO.,LIMITED
2026-06-26
Name:	Xiuying Zou		Function: Manager
Signature: [image: ]
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product:


 


Equipment


 


manufacturer


 


Shenzhen Doke Electronic Co.,


 


LTD


 


Type


 


XPLORE 6


,


 


XPLORE 6 Pro


 


Product description


 


Rugged Smartphone


 


HW versi


on


 


G2596


-


MS


-


V3.0


 


SW version


 


XPLORE6_EEA_G2596_V1.0_A16


 


 


Optional accessories or 


System components


 


Battery 


 


Model: Li536385HTT  


 


Rated Voltage: 7.6V
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E U Declaration   of   C onformi ty   (DoC)    

Company name  HONG KONG LELEGAO TECHNOLOGY CO.,LIMITED  

Postal a ddress  19H Maxgrand Plaza, No.3 Tai Yau Street, San Po Kong,  Kowloon, HongKong  

Postcode and City  HongKong  

Telephone number  +86 75532909320  

E - mail address  zxy@blackview.hk  

We declare that the DoC is issued under our sole responsibility and belongs to the following  product:  

Equipment   manufacturer  Shenzhen Doke Electronic Co.,   LTD  

Type  XPLORE 6 ,   XPLORE 6 Pro  

Product description  Rugged Smartphone  

HW versi on  G2596 - MS - V3.0  SW version  XPLORE6_EEA_G2596_V1.0_A16    

Optional accessories or  System components  Battery    Model: Li536385HTT     Rated Voltage: 7.6V   Charge Limit Voltage: 9.06V   Capacity: 6000mAh     Adapter    Model: HJPD120 - EU     Brand: Blackview    Input: 100 - 24 0V 50/60Hz 3.0A Max.     Output: USB - C:5.0V 3.0A(15.0W)or 9.0V 3.0A(27.0W) or    12.0V 3.0A(36.0W)or 15.0V 3.0A(45.0W) or 20.0V  6.0A(120.0W) (PPS)5.0V 20.0V 6.0A(120.0W Max)   Output USB - A: 5.0V 3.0A(15.0W) or 9.0V 3.0A(27.0W)or    12.0V 3.0A(36.0W)or 15.0V 3.0A(4 5.0W) or 20.0V 3.0A(60.0W)    (PPS)5.0V - 20.0V 3.0A(60.0W Max)  

  The object of the declaration described above is in conf ormity with the relevant Union  Harmonisation L egislation:  

RE Directive 2014/5 3 /EU   

  The  Notified Body Name:   LGAI Technological Center S.A ./Applus   (Nr. 0370) ,  has  conducted   the conformity assessment according to module B of Directive 2014/ 53/EU (RED) and issues  the EU  type certificate [ 0370 - RED - 12025 ].    

