
Declaration of Conformity (DoC)


We, Shenzhen Doke Electronic Co., LTD 
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China


Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Tablet PC

	Trademark：
	Blackview

	Model Number(s):
	ZENO 5



(Name of product, type or model, batch or serial number)


System components:

PIFA Antenna 
Bluetooth: 1dBi
2.4G WLAN: 1dBi
5.2G WLAN: 1dBi
5.8G WLAN: 1dBi
GSM 900: -1.10dBi; GSM 1800: 0.65dBi
WCDMA B1: 0.92dBi; WCDMA B8: -1.10dBi
LTE B1: 0.9dBi; LTE B3: 0.8dBi; LTE B7: 0.7dBi; LTE B8: -1.1dBi; LTE B20: -1.1dBi; ; LTE B28: -2dBi

Adapter:
Model: QZ-0180AEA00
Input: 100-240V~50/60Hz 0.5A 
[bookmark: _GoBack]Output: DC 5.0V 3.0A 15.0W orDC 9.0V 2.0A 18.0W or DC12.0V 1.5A 18.0W
Manufacturer: Guangdong Quanzhi Technology Co., Ltd.
Rechargeable Li-ion Battery:
Model: U3067133PHVUTL
Rated Voltage: 3.85V
Charge Limit Voltage: 4.4V
Capacity: 8300mAh
Manufacturer: SHENZHE NUTILITY ENERGY CO., LTD.

[image: ]
The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

HEALTH & SAFETY (Art. 3(1)(a)):

EN IEC 62368-1:2020+A11:2020

EN 50566: 2017+A1:2023

EN IEC/IEEE 62209-1528:2021

EN 50663:2017

EN 62479:2010

EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)

ETSI EN 301 489-3 V2.3.2 (2023-01)

ETSI EN 301 489-17 V3.3.1 (2024-09)

ETSI EN 301 489-19 V2.2.1 (2022-09)

ETSI EN 301 489-52 V1.3.1 (2024-11)

EN 55032:2015+A11:2020

EN IEC 61000-3-2:2019+A2:2024

EN 61000-3-3:2013+A2:2021+AC:2022

EN 55035:2017+A11:2020

Radio Spectrum (Article 3.2):

ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 300 440 V2.2.1 (2018-07)
ETSI EN 303 413 V1.2.1 (2021-04)
ETSI EN 303 345-1 V1.1.1(2019-06)
ETSI EN 303 345-3 V1.1.1(2021-06)
ETSI EN 301 511 V12.5.1 (2017-03)
ETSI EN 301 908-1 V15.2.1 (2023-01)
ETSI EN 301 908-2 V13.1.1 (2020-06)
ETSI EN 301 908-13 V13.3.1 (2024-10)
The submitted samples of the above equipment has been tested and found to comply with the following European Directives:
RoHS Directive 2011/65/EU & (EU) 2015/863

NOTIFIEDBODY:
Name: DERYCOM CERTIFICATION SERVICES, INC.
Address:1100  FalconAvenueGlencoe,Mn55336 IdentificationNumber:3052
EU-type examination certificate number: JEC-96

RF Specification:

	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	2.85 dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	3.5 dBm

	WIFI 802.11b/g/
n(HT20/40)
	802.11b/g/n(20MHz): 2412~2472MHz;
802.11n(40MHz):2422~2462MHz
	15.32dBm

	[bookmark: OLE_LINK14]Wi-Fi 5.2G(802.11a/n20/ac 20/
N40/ac40/ac80)
	802.11a/ n20/ac 20:5180MHz~5240MHz
802.11 n40/ac 40:5190MHz~5230MHz
802.11 ac 80:5210MHz
	14.23dBm

	Wi-Fi 5.8G(802.11a/n20/ac 20/
N40/ac40/ac80)
	802.11a/ n20/ac20:5745MHz~5825MHz
802.11 n40/ac40:5755MHz~5795MHz
802.11 ac 80:57750MHz
	12.95dBm

	GSM/GPRS 900
	TX(Uplink):880M‐915MHZ;
RX(Downlink):925M‐960MHZ
	33.21dBm

	GSM/GPRS 1800
	TX(Uplink):1710M‐1785MHZ;
RX(Downlink):1805M‐1880MHZ
	29.73 dBm

	WCDMA B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	22.10 dBm

	WCDMA B8
	TX(Uplink): 880-915MHz;
RX(Downlink):925-960MHz
	23.06dBm

	LTE FDD B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	22.53dBm

	LTE FDD B3
	TX(Uplink) :1710-1785MHz;
RX(Downlink):1805-1880MHz
	23.83 dBm

	LTE FDD B7
	TX(Uplink) :2500-2570MHz;
RX(Downlink):2620-2690MHz
	23.72 dBm

	LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz
RX(Downlink): 925 MHz to 960 MHz
	24.58dBm

	LTE FDD B20
	TX(Uplink): 832MHz~862MHz;
RX(Downlink):791MHz~821MHz
	23.82 dBm

	LTE FDD B28
	TX(Uplink):    703 MHz to 748MHz
RX(Downlink): 758 MHz to 803 MHz
	23.93dBm



Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position when used closet other body (at a minimum distance of 0mm) are:

	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	10-gBody
	0.863

	Limitis 4.0(W/kg) for10-g
	10-gMemberDAS
	0.863





Technical file held by: Shenzhen Doke Electronic Co., LTD 
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China  

Signed for and on behalf of:                           Shenzhen Doke Electronic Co., LTD
	Name and Title:
	

	Address:
	801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China  


[image: ]



Signature of Authorized Person
2026-04-27
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