
Declaration of Conformity (DoC)


[bookmark: We,_Shenzhen_Doke_Electronic_Co.,_LTD]We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Tablet PC

	Brand Name
	Blackview

	Model Number(s):
	                   MEGA 5

	Hardware Version:
	J50_T7300_D4UF

	Software Version:
	MEGA_5_EEA_j50

	Operating system:
	Android






(Name of product, type or model, batch or serial number)


System components:

FPC Antenna; 
gain: BT/Wi-Fi2.4G:2.13dBi;  WIFI5G:2.51dBi; 
GSM900:-1.12 dBi, DCS1800:0.33 dBi, WCDMA B1:0.53 dBi, WCDMA B8:-1.12 dBi,
LTE B1:0.53 dBi, LTE B3:0.33 dBi, LTE B7:0.62 dBi, LTE B8:-1.12 dBi, 
LTE B20:-1.34 dBi, LTE B28:-2.61 dBi
GPS: FPC Antenna
FM: Use earphone as Antenna



Adapter:
Model: QZ-05500EC00
Brand: Blackview
Input: 100-240V~50/60Hz 1.2A
Output: 5.0V[image: ] 2.0A or 5.0V [image: ]3A
(PPS)9-20V[image: ]3-2.75A
Manufacturer: Guangdong Quanzhi Technology
Co.,Ltd. 
Rechargeable Li-ion Battery:
Model: LiU3289113PHVUTL; Specification: DC 3.87V, 10000mAh, 38.7Wh
Manufacturer: SHENZHEN UTILITY ENERGY CO.,LTD

USB Cable: 110cm;


[image: ]

The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

[bookmark: HEALTH_&_SAFETY_(Art._3(1)(a)):]HEALTH & SAFETY (Art. 3(1)(a)):

EN 50566:2017;
EN 50566:2017/A1:2023
EN IEC/IEEE 62209-1528:2021
EN 62479:2010
EN IEC 62368-1:2020+A11:2020
[bookmark: EMC_(Art._3(1)(b)):]EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)
ETSI EN 301 489-3 V2.3.2 (2023-01)
ETSI EN 301 489-17 V3.3.1 (2024-09)
ETSI EN 301 489-19 V2.2.1 (2022-09)
ETSI EN 301 489-52 V1.3.1 (2024-11) EN 55032:2015+A11:2020
EN 55035:2017+A11:2020
EN IEC 61000-3-2:2019+A2:2024 EN 61000-3-3:2013+A2:2021+AC:2022

[bookmark: Radio_Spectrum_(Article_3.2):]Radio Spectrum (Article 3.2):

ETSI EN 301 511 V12.5.1 (2017-03);
TS 151 010-1 V13.14.0 (2024-06)
ETSI EN 301 908-1 V15.2.1 (2023-01)
ETSI EN 301 908-2 V13.1.1 (2020-06);
ETSI EN 301 908-13 V13.3.1 (2024-10)
ETSI EN 300 328 V2.2.2 (2019-07);
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 300 440 V2.2.1 (2018-07)
ETSI EN 303 413 V1.2.1 (2021-04) ;
ETSI EN 303 345-1 V1.1.1 (2019-06);
ETSI EN 303 345-3 V1.1.1 (2021-06)

The submitted samples of the above equipment has been tested and found to comply with the following European 
Directives: RoHS Directive 2011/65/EU & (EU) 2015/863




[bookmark: RF_Specification:]RF Specification:


	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	4.54 dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	3.86 dBm

	WIFI 802.11b/g/
n(HT20/40)
	802.11b/g/n(20MHz): 2412~2472MHz;
802.11n(40MHz):2422~2462MHz
	13.95dBm 

	Wi-Fi
5.2G(802.11a/n20/n40/ac2
0/ac40/ac80)
	802.11a/ n20/ac20:5180MHz~5240MHz
802.11 n40/ac40:5190MHz~5230MHz
802.11 ac80:5210MHz
	13.58dBm 

	Wi-Fi
5.8G(802.11a/n20/n40/ac2
0/ac40/ac80)
	802.11a/ n20/ac20:5745MHz~5825MHz
802.11 n40/ac40:5755MHz~5795MHz
802.11 ac80:57750MHz
	11.58 dBm 

	GSM/GPRS/EGPRS 900
	TX(Uplink):880M-915MHZ;
RX(Downlink):925M-960MHZ
	33.19 dBm 

	GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M-1785MHZ;
RX(Downlink):1805M-1880MHZ
	30.76 dBm  

	WCDMA B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	23.66 dBm  

	WCDMA B8
	TX(Uplink): 880-915MHz;
RX(Downlink):925-960MHz
	23.56 dBm  

	LTE FDD B1
	TX(Uplink):1920-1980MHz;
RX(Downlink):2110-2170MHz
	23.74 dBm

	LTE FDD B3
	TX(Uplink) :1710-1785MHz;
RX(Downlink):1805-1880MHz
	23.88  dBm

	LTE FDD B7
	TX(Uplink) :2500-2570MHz;
RX(Downlink):2620-2690MHz
	23.65  dBm

	LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz
RX(Downlink): 925 MHz to 960 MHz
	23.56  dBm

	LTE FDD B20
	TX(Uplink): 832MHz~862MHz;
RX(Downlink):791MHz~821MHz
	23.51 dBm

	LTE FDD B40
	Uplink & Downlink: 2300 MHz to 2400 MHz
	23.43dBm

	FM
	Rx(Downlink): 87.5MHz~108MHz
	--

	GPS
	Rx(Downlink): 1.57542GHz
	--



Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg) Limitis 2.0(W/kg) for10-g
	
Body
	
1.611W/kg

	Max SAR Value(W/kg) Limitis 4.0(W/kg) for10-g
	 Member DAS
	1.611W/kg





Technical file held by: Shenzhen Doke Electronic Co., LTD
Address: 801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Signed for and on behalf of:	Shenzhen Doke Electronic Co., LTD

	Name and Title:
	[bookmark: _GoBack]Xie ce / Manager

	Address:
	
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China







[bookmark: Signature_of_Authorized_Person]Signature of Authorized Person
2026-05-11
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  Decla r a t i o n   o f   C o n f o r m i t y   ( D o C)       We,  Shenzhen Doke Electronic Co., LTD   801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen,  China     Dec l ar e   t h a t   t he   D oC   is   i s s u e d   u nd e r   o ur   s ole   r es p o n s i b i l i t y   a nd   b e l o ngs   t o   t he   f o l l o w ing   p rod u c t (s ) :    

P r od u c t   T y p e:  Tablet PC  

Brand Name  Blackview  

Mod e l   N u m b e r(s ) :                      MEGA 5  

Hardware Version :  J50_T7300_D4UF  

Software Version:  MEGA_5_EEA_j50  

O perating system :  Android  

        (N a m e   o f   pr o du c t ,   t y p e   o r   m od e l,   b a t c h   o r   s e r i a l   n u m b er )       S y s t e m   c o m p o ne n ts :     FPC   A n t e nn a ;     ga i n :   B T / W i - F i 2.4 G : 2.13 d B i ;    W I F I5 G : 2. 51 d B i ;    GSM900: - 1.12 dBi ,  DCS1800:0.33 dBi ,  WCDMA B1:0.53 dBi ,  WCDMA B8: - 1.12 dBi ,   LTE B1:0.53  dBi ,  LTE B3:0.33 dBi ,  LTE B7:0.62 dBi ,  LTE B8: - 1.12 dBi ,    LTE B20: - 1.34 dBi ,  LTE B28: - 2.61 dBi   GPS:  FPC   Antenna   F M :   U s e   earph o n e   a s   A n t enna         A d a p t e r :   Model:   QZ - 05500EC00   Brand: Blackview   Input: 100 - 240V~50/60Hz 1.2A   Output: 5.0V   2.0A or 5.0V  3A   (PPS)9 - 20V 3 - 2.75A   M anu f a c t ure r :   Gu a ng d on g   Qu a n z h i   T e c h no l o g y   C o ., L t d .     R e c ha r ge a b le   L i - i o n   B a tt e r y :   M ode l:   LiU3289113PH VUTL ;   S p e c i f i c a ti o n :   D C   3 . 8 7 V,   10 00 0 mA h ,   3 8.7 W h   M anu f a c t ure r :   SHENZHEN UTILITY ENERGY  CO., LTD     U SB   Cab l e :   1 1 0 c m;      

