
Declaration of Conformity (DoC)


We, Shenzhen Doke Electronic Co., LTD
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Smartphone

	Trademark：
	Blackview

	Model Number(s):
	WAVE 10C


Operating system:

Hardware Version: 4+32: J567F_610_310_D3EF_V1.0
4+128: J567F_610_310_D4EF_V1.0

Software Version: WAVE10C_EEA_j567f_V1.0_A16

(Name of product, type or model, batch or serial number)


System components:，

FPC Antenna 
Bluetooth: 1.07dBi
2.4G WLAN: 1.07dBi
5.2G WLAN: 1.43dBi
5.8G WLAN: 1.43dBi
PIFA Antenna:  GSM 900: -0.31dBi; GSM 1800: -5.18dBi
WCDMA B1: 0.87dBi; WCDMA B8: -0.31dBi
LTE B1: 0.87dBi; LTE B3: -0.58dBi; LTE B7: -5.13dBi; LTE B8: -0.31dBi; LTE B20: -1.46dBi;

Adapter:
Model: QZ-01004EA00 
Input: 100-240V~50/60Hz 0.3A
Output: DC 5.0V 2.0A (10.0W)
Manufacturer: Guangdong Quanzhi Technology Co.,Ltd.

Model: HJ-0502000-EU
Input: 100-240V~ 50/60Hz 0.3A  
Output: DC 5.0V 2.0A 10.0W
Manufacturer: Shenzhen Huajin Electronics Co.,Ltd

Rechargeable Li-ion Battery:
Model: FHPV466495PNJ; Specification: DC 3.85V, 5000mAh 
Manufacturer: Shenzhen Nuojia Technology lndustrial Co., LTD
USB Cable: 100cm;


The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU).
The following harmonized standards and technical specifications have been applied:

HEALTH & SAFETY (Art. 3(1)(a)):

EN 50360:2017+A1:2023 EN 50566:2017+A1:2023 EN IEC/IEEE 62209-1528:2021 EN 50663:2017 EN 62479:2010 
EN IEC 62368-1:2020+A11:2020
EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)

ETSI EN 301 489-3 V2.3.2 (2023-01)

ETSI EN 301 489-17 V3.3.1 (2024-09)

ETSI EN 301 489-19 V2.2.1 (2022-09)

ETSI EN 301 489-52 V1.3.1 (2024-11)

EN 55032:2015+A11:2020; EN 55035:2017+A11:2020

EN IEC 61000-3-2:2019+A2:2024; EN 61000-3-3:2013+A2:2021+AC:2022

Radio Spectrum (Article 3.2):

ETSI EN 301 511 V12.5.1 (2017-03);

TS 151 010-1 V13.14.0 (2024-06)

ETSI EN 301 908-1 V15.2.1 (2023-01)

ETSI EN 301 908-2 V13.1.1 (2020-06)

ETSI EN 301 908-13 V13.3.1 (2024-10)

EN 300 328 V2.2.2 (2019-07);

EN 303 345-1 V1.1.1 (2019-06)

EN 303 345-3 V1.1.1 (2021-06)

EN 301 893 V2.1.1 (2017-05);

EN 300 440 V2.2.1 (2018-07);

EN 303 413 V1.2.1 (2021-04);


The submitted samples of the above equipment has been tested and found to comply with the following European Directives:
RoHS Directive 2011/65/EU & (EU) 2015/863

NOTIFIEDBODY:
Name:LGAI TECHNOLOGICAL CENTER, S.A. (APPLUS)
Address: Ronda de la Font del Carme, s/n 08193 Bellaterra – Barcelona (Spain) 
Notified Body No. 0370
EU-type examination certificate number: 0370-RED-12250


[bookmark: Notified_Body_Involved:]

RF Specification:


	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	0.84dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	2.14dBm

	WIFI 2.4G
802.11b/n(20MHz):
802.11n(40MHz):
	
802.11b/n(20MHz):2412-2472MHz
802.11n(40MHz):2422~2462MHz
	
13.71dBm

	[bookmark: OLE_LINK14]Wi-Fi 5.2G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac(80MHz):
	
802.11a/n/ac (20MHz):5180~5240MHZ
802.11n/ac(40MHz):5190~5230MHZ
802.11ac(80MHz):5210MHz
	


13.97dBm

	Wi-Fi 5.8G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac (80MHz):
	
802.11a/n/ac(20MHz):5745~5825MHz
802.11n /ac(40MHz):5755~5795MHz
802.11ac (80MHz):5775MHz
	


11.92dBm

	
GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;

RX(Downlink):925M‐960MHZ
	
33.42dBm

	
GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;

RX(Downlink):1805M‐1880MHZ
	
30.99dBm

	
WCDMA B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
23.49dBm

	
WCDMA B8
	TX(Uplink): 880-915MHz;

RX(Downlink):925-960MHz
	
23.09dBm

	
LTE FDD B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
23.49dBm

	
LTE FDD B3
	TX(Uplink) :1710-1785MHz;

RX(Downlink):1805-1880MHz
	
23.45dBm

	
LTE FDD B7
	TX(Uplink) :2500-2570MHz;

RX(Downlink):2620-2690MHz
	
22.84dBm

	
LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz

RX(Downlink): 925 MHz to 960 MHz
	
22.87dBm

	
LTE FDD B20
	TX(Uplink): 832MHz~862MHz;

RX(Downlink):791MHz~821MHz
	
22.74dBm

	GPS
	[bookmark: _GoBack]Rx(Downlink): 1.57542GHz
	--

	FM
	Rx(Downlink): 87.5-108MHZ
	--








Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	10g-Head
	0.922W/kg

	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	10g-Body
	1.769W/kg

	Limitis 4.0(W/kg) for10-g
	Member DAS
	1.769W/kg





Technical file held by: Shenzhen Doke Electronic Co., LTD

801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China

Signed for and on behalf of:                           Shenzhen Doke Electronic Co., LTD


	Name and Title:
	Duan chunlin/Manager

	Address:
	801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China
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