**Declaration of Conformity (DoC)**

We,**Shenzhen DOKE Electronic Co.,Ltd.**

801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China.

**Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):**

|  |  |
| --- | --- |
| **Product Type:** | **Mobile Phone** |
| **Trademark：** | **Blackview, OSCAL** |
| **Model Number(s):**  | **SHARK 6, TIGER 8** |
|  |  |

|  |
| --- |
| (Name of product, type or model, batch or serial number)System components:For BT/BLE/2.4G WIFI/5G WIFI/NFC/GNSS/GSM/WCDMA/LTE/5G NR: FPC AntennaFor FM: Integral Antenna/BT/BLE/2.4G WIFI: 0.66dBi5G WIFI: 1.62dBiE-GSM 900/GPRS 900/EGPRS 900: -2.82dBiGSM 1800/GPRS 1800/EGPRS 1800: 0.77dBi WCDMA Band I: 0.66dBiWCDMA Band VIII: -2.82dBiLTE band 1: 0.66dBi LTE band 3: 0.77dBiLTE band 7: 2.33dBi LTE band 8: -2.82dBiLTE band 20: -1.77dBi LTE band 28: -3.18dBiNR n1: 0.66dBiNR n3: 0.77dBiNR n8: -2.82dBiNR n20: -1.77dBiNR n28: -3.18dBiNR n40: 1.78dBi NR n77: -0.72dBiNR n78: 0.82dBi**Adapter Information:**Model: QZ-0180AEA00Input: AC 100-240V, 50/60Hz, 0.5AOutput: DC 5.0V, 3.0A, 15.0W or DC 9.0V, 2.0A, 18.0W or DC 12.0V, 1.5A, 18.0WManufacturer: Guangdong Quanzhi Technology Co.,Ltd.Rechargeable Li-ion Battery:Model: Li456788PLGY; Specification: 3.89V, 5000mAh, 19.45Wh;Manufacturer: Hunan Gaoyuan Battery Co., Ltd.USB Cable:100cm**The object of the declaration described above is in conformity with the essential requirements of the relevant Union harmonization legislation: Radio Equipment Directive *RED (2014/53/EU)*.** **The following *harmonized* standards and technical specifications have been applied:** **HEALTH & SAFETY (Art. 3(1)(a)):**EN 50566:2017+A1:2023 EN 50663:2017EN IEC/IEEE 62209-1528:2021 EN 50360:2017+A1:2023 EN 62479:2010EN IEC 62311:2020EN IEC 62368-1:2020+A11:2020**EMC (Art. 3(1)(b)):** ETSI EN 301 489-52 V1.3.1 (2024-11)ETSI EN 301 489-19 V2.2.1 (2022-09)ETSI EN 301 489-17 V3.3.1 (2024-09)ETSI EN 301 489-3 V2.3.2 (2023-01)ETSI EN 301 489-1 V2.2.3 (2019-11)EN 55032:2015+A11:2020+A1:2020EN 55035:2017+A11:2020EN IEC 61000-3-2:2019+A1:2021EN 61000-3-3:2013+A1:2019+A2:2021**Radio Spectrum (Article 3.2):**ETSI EN 300 328 V2.2.2 (2019-07)ETSI EN 301 893 V2.1.1 (2017-05)ETSI EN 300 440 V2.2.1 (2018-07)ETSI EN 300 330 V2.1.1 (2017-02)ETSI EN 303 413 V1.2.1 (2021-04)ETSI EN 303 345-1 V1.1.1 (2019-06)ETSI EN 303 345-3 V1.1.1 (2021-06)ETSI EN 301 511 V12.5.1 (2017-03)ETSI EN 301 908-1 V15.2.1 (2023-01)ETSI EN 301 908-2 V13.1.1 (2020-06)ETSI EN 301 908-13 V13.2.1 (2022-02)ETSI EN 301 908-25 V15.1.1 (2024-10)ETSI TS 138 521-1 V17.11.0 (2024-01)ETSI TS 138 521-3 V17.11.0 (2024-01) |

**Notified Body Involved:**

Notified Body Name: DERYCOM CERTIFICATION SERVICES, INC.

Notified Body Number: 3052

Notified Body Assessment Performed: Module B/C on Article 3.1a, 3.1b, 3.2

EU-type examination certificate number:  TCT-96

RF Specification:

|  |  |  |
| --- | --- | --- |
| **Function** | **Operation Frequency** | **Max RF output power:** |
| BLE | 2402MHz–2480MHz | -0.29 dBm |
| BT(BR+EDR) | 2402MHz–2480MHz | 7.64 dBm |
| WIFI 802.11b/g/n(HT20/40) | 802.11b/g/n(20MHz): 2412~2472MHz;802.11n(40MHz):2422~2462MHz | 17.89 dBm |
| Wi-Fi5.2G(802.11a/n20/n40/ac20/ac40/ac80) | 5150MHz~5250MHz | 13.55 dBm |
| Wi-Fi5.8G(802.11a/n20/n40/ac20/ac40/ac80) | 5725MHz~5875MHz | 12.40 dBm |
| GSM/GPRS/EGPRS 900 | TX:880M‐915MHZ;RX:925M‐960MHZ | 33.26 dBm |
| GSM/GPRS/EGPRS 1800 | TX:1710M‐1785MHZ;RX:1805M‐1880MHZ | 30.28 dBm  |
| WCDMA B1 | TX:1920-1980MHz;RX:2110-2170MHz | 23.47 dBm  |
| WCDMA B8 | TX: 880-915MHz;RX:925-960MHz | 23.06 dBm  |
| LTE FDD B1 | (UL)1920MHz~1980MHz,(DL)2110MHz~2170MHz | 23.03 dBm  |
| LTE FDD B3 | (UL)1710MHz~1785MHz,(DL)1805MHz~1880MHz | 24.03 dBm  |
| LTE FDD B7 | (UL)2500MHz~2570MHz,(DL)2620MHz~2690MHz | 22.33 dBm  |
| LTE FDD B8 | (UL)880MHz~915MHz,(DL)925MHz~960MHz | 22.83 dBm  |
| LTE FDD B20 | (UL)832MHz~862MHz,(DL)791MHz~821MHz | 23.31 dBm |
| LTE FDD B28 | (UL)703MHz~748MHz,(DL)758MHz~803MHz | 23.16 dBm |
| NR n1 | (UL)1920MHz~1980MHz, (DL)2110MHz~2170MHz | 23.59 dBm |
| NR n3 | (UL)1710MHz~1785MHz, (DL)1805MHz~1880MHz | 24.76 dBm |
| NR n8 | (UL)880MHz~915MHz, (DL)925MHz~960MHz | 23.12 dBm |
| NR n20 | (UL)832MHz~862MHz, (DL)791MHz~821MHz | 24.82 dBm |
| NR n28 | (UL)703MHz~748MHz, (DL)758MHz~803MHz | 24.24 dBm |
| NR n40 | (UL)2300MHz~2400MHz, (DL)2300MHz~2400MHz | 24.77 dBm |
| NR n77 | (UL)3300MHz~4200MHz, (DL)3300MHz~4200MHz | 25.88 dBm |
| NR n78 | (UL)3300MHz~3800MHz, (DL)3300MHz~3800MHz | 25.43 dBm |
| NFC | 13.56MHz | -23.09 dBuA@10m |
| FM | Rx: 87.5MHz~108MHz | -- |
| GPS | Rx: 1.57542GHz | -- |
| BDS | Rx:1.561098GHz |  |
| Galileo | Rx:1.561098GHz |  |

Tests for SAR are conducted using standard operating positions with the device transmitting at its highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used close to the body (at a minimum distance of 5mm/0mm) are:

|  |  |  |
| --- | --- | --- |
| Max SAR Value(W/kg)Limit is 2.0(W/kg) for 10-g | 10-g Head | **0.28** W/kg |
| 10-g Body | **0.53** W/kg |
| Limit is 4.0(W/kg) for 10-g | 10-g Member DAS | **1.38** W/kg |

Technical file held by:Shenzhen DOKE Electronic Co., Ltd

801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China.

**Signed for and on behalf of:** Shenzhen DOKE Electronic Co., Ltd

|  |  |
| --- | --- |
| **Name and Title:**  | zhang.liuwei/Manager |
| **Address:**  | 801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China. |



Signature of Authorized Person

2025-06-17