
Declaration of Conformity (DoC)


We, Shenzhen Doke Electronic Co., LTD

801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, 
Shenzhen, China

Declare that the DoC is issued under our sole responsibility and belongs to the following product(s):

	Product Type:
	Smart tablet

	Brand Name
	Blackview

	Model Number(s):
	LINK Mini Kids

	Hardware Version:
	/

	Software version:
	/





(Name of product, type or model, batch or serial number)


System components:

PIFA antenna; 
Antenna Gain: 
BT/Wi-Fi2.4G: 0.8dBi;
WIFI5G: 1.2dBi; 



Adapter:
Model:QZ-01004EA00
Brand: Blackview
Input: 100-240V~50/60Hz 0.3A
Output: DC5.0V 2.0A 10.0W
Manufacturer: Quanzhi Guangdong Technology Co., Ltd.

Rechargeable Li-ion Battery:
Model: U317296PVUTL
Specification: 3.8V, 3000mAh, 11.4Wh
 Manufacturer: SHENZHEN UTILITY ENERGY CO., LTD.




[image: ]
The object of the declaration described above is in conformity with the essential requirements of

the relevant Union harmonization legislation: Radio Equipment Directive RED (2014/53/EU). The following harmonized standards and technical specifications have been applied: HEALTH & SAFETY (Art. 3(1)(a)):
EN 50566:2017+A1:2023
EN IEC/IEEE 62209-1528:2021
EN 50663:2017 
EN 62479:2010

EN IEC 62368-1:2020+A11:2020

EMC (Art. 3(1)(b)):

ETSI EN 301 489-1 V2.2.3 (2019-11)
ETSI EN 301 489-3 V2.3.2 (2023-01)
ETSI EN 301 489-17 V3.3.1 (2024-09)
EN 55032:2015+A11:2020
EN 55035:2017+A11:2020
EN IEC 61000-3-2:2019+A2:2024 
EN 61000-3-3:2013+A2:2021+AC:2022

Radio Spectrum (Article 3.2):

ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 300 440 V2.2.1 (2018-07)


The submitted samples of the above equipment has been tested and found to comply with the following European Directives:
RoHS Directive 2011/65/EU & (EU) 2015/863


NOTIFIEDBODY:
[bookmark: Name:DERYCOM_CERTIFICATION_SERVICES,_INC]Name: LGAl Technological Center S.A. (APPLUS)

Address: Campus UAB. Ronda de la Font del Carme s/n08193 Bellaterra, Barcelona (Spain)

 Notified Body No. 0370

EU-type examination certificate number: No. 0370-RED-11558

RF Specification:

	Function
	OperationFrequency
	Max RF output power:

	BLE 
	2402MHz–2480MHz
	2.42dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	2.50dBm

	WIFI 802.11b/g/
n(HT20/40)/ ax(HE20/40)
	802.11b/g/n(20MHz)/ax(20MHz):2412~2472MHz;
802.11n(40MHz)/ax(40MHz):2422~2462MHz
	13.80dBm

	Wi-Fi
5.2G(802.11a/n20/n40/ac2
0/ac40/ax20/ax40
	802.11a/n20/ac20/ ax20:5180MHz~5240MHz
802.11 n40/ac40/ax40:5190MHz~5230MHz

	13.90dBm

	Wi-Fi
5.8G(802.11a/n20/n40/ac2
0/ac40/ax20/ax40
	802.11a/n20/ac20/ax20:5745MHz~5825MHz
802.11n40/ac40/ax20:5755MHz~5795MHz

	13.59dBm




Tests for SAR are conducted using standard operating positions with the device transmitting at its

highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:

	Max SAR Value(W/kg) Limitis 2.0(W/kg) for10-g
	
Body
	
0.174W/kg

	Max SAR Value(W/kg) Limitis 4.0(W/kg) for10-g
	Member DAS
	0.174W/kg





Technical file held by: Shenzhen Doke Electronic Co., LTD
Address: 801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China
Signed for and on behalf of:	Shenzhen Doke Electronic Co., LTD

	Name and Title:
	Hong zongqing / Manager

	Address:
	
801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District, Shenzhen, China




[image: ]


Signature of Authorized Person
[bookmark: _GoBack]2026-05-08
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  Decl a r ation   o f   C o nfo r m i t y   (DoC)       W e ,   Shenzhen Doke Electronic Co., LTD     801, Building3, 7th Industrial Zone, Yulv Community, Yutang Road, Guangming District,    Shenzhen, China     Dec l ar e   t hat   t he   D oC   is   i s s u e d   u nder   o ur   s ole   r es p o n s i b i l i t y   a nd   b e l o ngs   t o   t he   f o l l o w ing   p rod u c t (s ) :    

Product Type:  Smart tablet  

Brand Name  Blackview  

Model Number(s):  LINK Mini Kids  

Hardware Version :  /  

Software  v ersion :  /  

      (N a m e   o f   pr o du c t ,   t y p e   o r   m od e l,   b a tch   o r   s e r ial   n u m b er )       S y s t e m   c o m p o ne n ts:     PIFA   antenna ;     Antenna Gain :     B T / W i - F i 2.4 G :   0.8 d B i ;   W I F I5 G :   1.2 d B i ;          A d a p t e r :   Model:QZ - 01004EA00   Brand: Blackview   Input: 100 - 240V~50/60Hz 0.3A   Output: DC5.0V   2.0A 10.0W   Manufa c turer:  Quanzhi   Guangdong   Technology Co., Ltd.     Rechargeable Li - ion Battery:   Model:  U317296PVUTL   Specification:  3.8V,   3000mAh ,  11.4Wh     Manufacturer:  SHENZHEN   UTILITY ENERGY   CO., LTD.        

