EU Declaration of Conformity (DoC)
	Company name
	HONG KONG LELEGAO TECHNOLOGY CO.,LIMITED

	Postal address
	19H Maxgrand Plaza, No.3 Tai Yau Street, San Po Kong, Kowloon, HongKong 

	Postcode and City
	 HongKong

	Telephone number
	+86 0755-32909316

	E-mail address
	xiece@blackview.hk



We declare that the DoC is issued under our sole responsibility and belongs to the following product:
	Equipment manufacturer
	Shenzhen Doke Electronic Co., LTD 

	Type
	XPLORE X1, XPLORE X1 Pro 

	Product description
	Smart Phone with GSM, Bluetooth, WiFi, WCDMA, GPS, LTE, 5G_NR, FM, NFC

	HW version
	F253-V1.2
	SW version
	XPLORE_X1_EEA_F253

	Optional accessories or System components
	




The object of the declaration described above is in conformity with the relevant Union Harmonisation Legislation:
	RE Directive 2014/53/EU
	

	Directive 2011/65/EU
	

	
	



The submitted samples of the above equipment has been tested and found to comply with the following European Directives: RoHS Directive 2011/65/EU & (EU) 2015/863.

[bookmark: OLE_LINK1]The Notified Body Name: LGAI Technological Center S.A./Applus (Nr. 0370), has conducted the conformity assessment according to module B of Directive 2014/53/EU (RED) and issues the EU type certificate [0370-RED-11866].

The following standards and technical specifications have been applied for RE Directive 2014/53/EU:
	Article 3.1a: Safety and Health
	EN IEC 62368-1:2024+A11:2024
EN 50360: 2017+A1:2023
EN 50566: 2017+A1:2023
EN IEC/IEEE 62209-1528:2021
EN 50663:2017; EN 62479:2010

	Article 3.1b: EMC
	ETSI EN 301 489-1 V2.2.3 (2019-11) 
ETSI EN 301 489-3 V2.3.2 (2023-01)
ETSI EN 301 489-17 V3.3.1 (2024-09)
ETSI EN 301 489-19 V2.2.1 (2022-09)
ETSI EN 301 489-52 V1.3.1 (2024-11) 
EN 55032:2015+A11:2020
EN IEC 61000-3-2:2019+A2:2024
EN 61000-3-3:2013+A2:2021+AC:2022
EN 55035:2017+A11:2020

	Article 3.2: RF Spectrum Efficiency
	ETSI EN 300 328 V2.2.2 (2019-07)
ETSI EN 301 893 V2.1.1 (2017-05)
ETSI EN 300 440 V2.2.1 (2018-07)
ETSI EN 303 413 V1.2.1 (2021-04)
ETSI EN 303 345-1V1.1.1(2019-06)
ETSI EN 303 345-3V1.1.1(2021-06)
ETSI EN 301 511 V12.5.1 (2017-03)
ETSI TS 151 010-1 V13.14.0(2024-06)
ETSI EN 301 908-1 V15.2.1 (2023-01)
ETSI EN 301 908-2 V13.1.1 (2020-06)
ETSI EN 301 908-13 V13.3.1 (2024-10)
ETSI TS 138 521-1 V17.6.1 (2022-10)
ETSI TS 138 521-3 V17.7.0 (2023-01)
ETSI EN 301 908-1 V15.2.1 (2023-01)
ETSI EN 301 908-25 V15.1.1 (2024-10)
EN 300 330 V2.1.1 (2017-02)

	Article 3.3: Special requirements invoked
	Not applicable



RF Specification: 

	Function
	Operation Frequency
	Max RF output power:

	BLE
	2402MHz–2480MHz
	2.09 dBm

	BT(BR+EDR)
	2402MHz–2480MHz
	3.56dBm

	WIFI 2.4G
802.11b/n(20MHz):
802.11n(40MHz):
	
802.11b/n(20MHz):2412-2472MHz
802.11n(40MHz):2422~2462MHz
	
13.84dBm

	[bookmark: OLE_LINK14]Wi-Fi 5.2G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac(80MHz):
	
802.11a/n/ac (20MHz):5180~5240MHZ
802.11n/ac(40MHz):5190~5230MHZ
802.11ac(80MHz):5210MHz
	


13.75dBm

	Wi-Fi 5.8G
802.11a/n/ac (20MHz):
802.11n/ac(40MHz):
802.11ac (80MHz):
	
802.11a/n/ac(20MHz):5745~5825MHz
802.11n /ac(40MHz):5755~5795MHz
802.11ac (80MHz):5775MHz
	


12.61dBm

	
GSM/GPRS/EGPRS 900
	TX(Uplink):880M‐915MHZ;

RX(Downlink):925M‐960MHZ
	
33.56dBm

	
GSM/GPRS/EGPRS 1800
	TX(Uplink):1710M‐1785MHZ;

RX(Downlink):1805M‐1880MHZ
	
30.19dBm

	
WCDMA B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
23.85 dBm

	
WCDMA B8
	TX(Uplink): 880-915MHz;

RX(Downlink):925-960MHz
	
23.15dBm

	
LTE FDD B1
	TX(Uplink):1920-1980MHz;

RX(Downlink):2110-2170MHz
	
21.75 dBm

	
LTE FDD B3
	TX(Uplink) :1710-1785MHz;

RX(Downlink):1805-1880MHz
	
22.29 dBm

	
LTE FDD B7
	TX(Uplink) :2500-2570MHz;

RX(Downlink):2620-2690MHz
	
21.83 dBm

	
LTE FDD B8
	TX(Uplink): 880MHz to 915 MHz

RX(Downlink): 925 MHz to 960 MHz
	
22.67dBm

	
LTE FDD B20
	TX(Uplink): 832MHz~862MHz;

RX(Downlink):791MHz~821MHz
	
22.34 dBm

	
LTE FDD B28
	TX(Uplink):    703 MHz to 748MHz

RX(Downlink): 758 MHz to 803 MHz
	
24.42 dBm

	SA N1
	1920-1980 MHz (TX), 2110-2170 MHz (RX)
	
22.01 dBm

	SA N3
	1710-1785 MHz (TX), 1805-1880 MHz (RX)
	
22.14 dBm

	SA N8
	880-915 MHz (TX), 925-960 MHz (RX)
	
22.91 dBm

	SA N20
	832-862 MHz (TX), 791-821 MHz (RX)
	
22.96 dBm

	SA N28
	703-748 MHz (TX), 758-803 MHz (RX)
	
22.68 dBm

	SA N40
	2300-2400 MHz (TX), 2300-2400 MHz (RX)
	
22.91dBm

	SA N77
	3700-3800 MHz (TX), 3700-3800 MHz (RX)
	
25.89dBm

	[bookmark: _GoBack]SA N78
	3300-3800MHz(TX), 3300-3800MHz(RX)
	25.65 dBm

	GPS
	Rx(Downlink): 1.57542GHz
	--

	FM
	Rx(Downlink): 87.5-108MHZ
	--

	NFC
	13.56 MHz
	-22.15 dBuA/m @10m





Tests for SAR are conducted using standard operating positions with the device transmitting at its highest certified power level in all tested frequency bands. The maximum SAR values tested on this device when used in its normal position at the ear and when used closet othe body(at a minimum distance of 5mm/0mm) are:
	Max SAR Value(W/kg)

Limitis 2.0(W/kg) for10-g
	10g-Head
	0.457W/kg

	Limitis 4.0(W/kg) for10-g
	10g-Body/MemberDAS
	1.896W/kg



Signed on behalf of:	Shenzhen Doke Electronic Co., LTD
HongKong, 2026-06-10
Name:	Xie ce		Function: Manager
Signature: [image: ]
image1.png
X ce
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